{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["询价单"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"询价单","index":0,"n_rows":23,"n_cols":13,"rows_kept":23,"cut":false,"hidden":false,"merged":[[1,0,1,3],[1,6,1,11],[2,0,2,3],[2,6,2,11],[3,0,3,3],[3,6,3,11],[4,0,4,3],[4,6,4,11],[0,0,0,11]],"flags":["formulas_cached_only"]}
["锡林郭勒苏能正镶新能源有限公司物资采购询（报）价单"]
["报价单位（公章或合同章）:",{"$nulls":5},"询价部门："]
["联系人:",{"$nulls":5},"联系方式："]
["传真:",{"$nulls":5},"报价截止日期："]
["供应商编码:"]
["序号","物资编码","物资名称","规格","型号","计量单位","数量","交货期","主机","无税单价（元）","总价（元）","品牌","备注"]
["1","TM202505131009128830d70","智能球形摄像机","不低于200万像素；符合IP66防尘，支持3D数字降噪、强光抑制，支持玻璃加热除雾，支持宽动态范围达120dB，适合逆光环境监控","不低于200万像素；符合IP66防尘，支持3D数字降噪、强光抑制，支持玻璃加热除雾，支持宽动态范围达120dB，适合逆光环境监控","个","16.00","","","","","","16"]
["2","TM2025051310091288588b8","供电电池","摄像机需配置可拆卸锂电池，配置不少于2块，单块供电时间不低于8小时，需具备防水功能，电池需配备专用充电器16套。","摄像机需配置可拆卸锂电池，配置不少于2块，单块供电时间不低于8小时，需具备防水功能，电池需配备专用充电器16套。","个","32.00","","","","","","32"]
["3","TM2025051310091288645f8","摄像机立杆","不低于2米圆形杆。镀锌钢管，厚度1.7mm。","不低于2米圆形杆。镀锌钢管，厚度1.7mm。","套","12.00","","","","","","12"]
["4","TM202505131009128864d4d","执法记录仪","设备可录制存储视频，内存为128G。","设备可录制存储视频，内存为128G。","个","10.00","","","","","","10"]
["5","TM202505131009128874ec3","升压站摄像机立杆","需根据升压站围墙高度制定立杆","需根据升压站围墙高度制定立杆","个","4.00","","","","","","4"]
["6","TM202505131009128889575","2米立杆基础","基础由型钢或者钢板焊接而成，基础上设置压块保证摄像头稳定性与安全性，压块数量根据稳定性与安全性要求确定，单块压块满足单人可搬运且单块重量小于20Kg","基础由型钢或者钢板焊接而成，基础上设置压块保证摄像头稳定性与安全性，压块数量根据稳定性与安全性要求确定，单块压块满足单人可搬运且单块重量小于20Kg","个","16.00","","","","","","16"]
["7","TM202505131009128897be5","物联网卡","移动4G物联网卡","移动4G物联网卡","个","16.00","","","","","","16"]
["8","TM2025051310091289084e4","固态硬盘","4TB硬盘","4TB硬盘","块","10.00","","","","","","10"]
["9","TM20250513100912891fab1","配套设备及辅材","连接件、拉线等","连接件、拉线等","项","1.00","","","","","","1"]
["10","TM202505131009128924ae4","实施服务费","物流、施工安装、设备调试、培训工作、维护工作等","物流、施工安装、设备调试、培训工作、维护工作等","项","1.00","","","","","","1"]
["11","TM20250513115911127ecfb","SD卡","256G","256G","张","16.00","","","","","","16"]
["","合计","","","","","","","","","","",""]
["注：A、报价：无税单价（运费、装卸费出卖人承担）。"]
[" B、质量标准：国标、行业标准、企标，并注明标准号。非标产品以双方认可的图纸、协议等为准。"]
[" C、请务必填写完整、清晰，否则报价无效，修改处签章。"]
[" D、 “报价单”视为合同附件，具有法律效应。"]
[" E、付款方式：电子承兑。"]