{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["询价单"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"询价单","index":0,"n_rows":28,"n_cols":13,"rows_kept":28,"cut":false,"hidden":false,"merged":[[1,0,1,3],[1,6,1,11],[2,0,2,3],[2,6,2,11],[3,0,3,3],[3,6,3,11],[4,0,4,3],[4,6,4,11],[0,0,0,11]],"flags":["formulas_cached_only"]}
["江苏徐矿能源股份有限公司物资供销分公司物资采购询（报）价单"]
["报价单位（公章或合同章）:",{"$nulls":5},"询价部门："]
["联系人:",{"$nulls":5},"联系方式："]
["传真:",{"$nulls":5},"报价截止日期："]
["供应商编码:"]
["序号","物资编码","物资名称","规格","型号","计量单位","数量","交货期","主机","含税单价（元）","总价（元）","品牌","备注"]
["1","TM202505161656336290ce6","氧气减压器","YQY-07 2.5*25MPa","","套","5.00","","","","","",""]
["2","TM202505161656336331796","乙炔减压器","YQE-03 0.25*4MPa","","只","5.00","","","","","",""]
["3","TM2025051616563363716d0","防火毯","单层石棉 4m*1.5m*5mm","","张","10.00","","","","","",""]
["4","TM202505161656336415332","小型配电箱","HT-5WAY 长110X153X90mm 配置：防水配电箱X1 DZ47X 五孔16AX1 DZ47sL-2P 16A","","个","15.00","","","","","","电气：化学试验班标准化整改/"]
["5","TM20250516165633645f58c","不锈钢检修电源箱","尺寸：600*500*260额定电流：100A 额定电压：380v 配置：1、32A 4芯 2个 2、16A3芯220V 1个 3、10A5眼220v 1个","","个","1.00","","","","","","斗轮机检修电源箱更换/"]
["6","TM20250516165633649a425","接线端子","UK2.5N 侧厚5mm","","片","100.00","","","","","","皮带就地控制箱/"]
["7","TM202505161656336539d68","电缆","ZRC-VV-1-3×2.5 MM2","","m","200.00","","","","","","翻车机使用/"]
["8","TM20250516165633658d456","不锈钢端子箱","300*200*100mm 内含20片端子","","个","7.00","","","","","","#2皮带拉绳跑偏开关改造用/"]
["9","TM2025051616563366202b2","空气开关","NXBLE-32 2P 6A","","个","10.00","","","","","","热控：现场控制柜使用/"]
["10","TM202505161656336660197","空气开关","NXBLE-32 2P 10A","","个","10.00","","","","","","热控：现场控制柜使用/"]
["11","TM20250516165633673f6e9","防爆温度计","防爆型双金属温度计或一体化防爆数显热电阻：M27*2外螺纹，插深50mm，-20℃-50℃及以上 介质氢气，耐压至少6MPa","","支","3.00","","","","","","热控：制氢站安全整改使用3支/"]
["12","TM20250516165633679e979","寻线仪","型号：寻线仪多功能网络/电话测试仪/智能寻线对线 60B 模拟信号寻线","","个","1.00","","","","","","通讯专业：检修维护测线使用/"]
["13","TM202505161656336847790","荧光粉检测手电","120W 工业级 UV-365nm 含充电器","","把","2.00","","","","","","机务：输灰漏点检测使用/"]
["14","TM20250516165633688a01e","激光笔","蓝光 功率3-5W 光波455-450nm 含充电器","","把","2.00","","","","","","机务：查找漏点使用/"]
["15","TM20250516165633692d63a","密封条","D-05 U型顶泡 材质EPDM 黑色","","m","100.00","","","","","","电气和热控：现场配电柜、端子箱密封/"]
["16","TM20250516165633696a96e","保护罩（方形）","外部尺寸：长170mm*宽120mm*高70mm 厚度:2mm 材质：亚克力透明 五面","","个","2.00","","","","","","热控：澡堂供汽供水电磁阀线圈使用/"]
["","合计","","","","","","","","","","",""]
["注：A、报价：无税单价（运费、装卸费出卖人承担）。"]
[" B、质量标准：国标、行业标准、企标，并注明标准号。非标产品以双方认可的图纸、协议等为准。"]
[" C、请务必填写完整、清晰，否则报价无效，修改处签章。"]
[" D、 “报价单”视为合同附件，具有法律效应。"]
[" E、付款方式：电子承兑。"]