{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["询价单"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"询价单","index":0,"n_rows":30,"n_cols":13,"rows_kept":30,"cut":false,"hidden":false,"merged":[[1,0,1,3],[1,6,1,11],[2,0,2,3],[2,6,2,11],[3,0,3,3],[3,6,3,11],[4,0,4,3],[4,6,4,11],[0,0,0,11]],"flags":["formulas_cached_only"]}
["江苏徐矿能源股份有限公司物资供销分公司物资采购询（报）价单"]
["报价单位（公章或合同章）:",{"$nulls":5},"询价部门："]
["联系人:",{"$nulls":5},"联系方式："]
["传真:",{"$nulls":5},"报价截止日期："]
["供应商编码:"]
["序号","物资编码","物资名称","规格","型号","计量单位","数量","交货期","主机","含税单价（元）","总价（元）","品牌","备注"]
["1","TM20250711160547139a335","行车手柄","cob64带急停按钮","","个","2.00","","","","","","机务：#1、2引风机房起重设备使用"]
["2","TM2025071116054714147b0","304不锈钢工业检修插座箱","KMW58105 总漏保：100A 4P 1个 分空开：25A 1P 3个 分空开：63A 3P 3个 民用插座 220V 10A 5孔 3个 五芯插座 380V 32A 3个 下进线孔M36 配防水接头 配套插头各3个 IP54 壁挂式 外形尺寸：550*500*180mm 执行标准：GB7251.3\"","","个","17.00","","","","","","电气：全厂检修箱更换，含4个FJ6/JTS2接线端子(一进三出 出线孔径φ10mm)"]
["3","TM20250711160547143d350","开关电源","SFLD-030-1H 输入：100-240V 输出：DC12V 3A 外形尺寸：88*85*38mm","","块","2.00","","","","","","热控：#1炉、#2炉火焰电视监控使用2个/"]
["4","TM202507111605471444ecd","电源模块","输入：100-240V 频率50-60Hz 输出:5V 1A","","个","5.00","","","","","","热控：锅炉火焰电视监控及其他现场使用/"]
["5","TM20250711160547144d93c","电源模块","输入：100-240V 频率50-60Hz 输出:5V 2A","","个","5.00","","","","","","热控：锅炉云母水位计监控及其他现场使用/"]
["6","TM2025071116054714555d9","控制箱","深度150mm 宽度300mm 高度400mm 304材质 带把手门锁 柜门带“红”色380v指示灯 控制箱外有“有电危险”标识 ,厚度≧1mm 壁挂式安装 IP44","","个","8.00","","","","","","热控材料：磨煤机防爆蒸汽电动执行机构使用/"]
["7","TM202507111605471463577","航空插座","母头：Type：DEP2-325；32A-6h/415V~；3P+N+地线；IP44；GB/T11918.1 GB/T11918.2","","个","6.00","","","","","","机务：现场检修箱修旧利废使用/"]
["8","TM20250711160547147dec6","电磁阀","ZW-16C，PN16，DN50 压力：1.6Mpa 温度≤80℃， 线圈电压：DC24V","","个","1.00","","","","","","热控材料:住宅楼换热站低区电磁泄压阀/"]
["9","TM202507111605471483521","电磁阀","规格型号：ZCZP-16T 管径：DN50，阀体材质：铜 ，连接形式：螺纹，功能作用：快速型，压力环境：常压 ，线圈电压：DC24V，（阀体长度不带螺纹13cm）","","个","1.00","","","","","","热控材料:住宅楼换热站补水箱补水电磁阀/"]
["10","TM202507111605471492c43","户外型不锈钢工业检修插座箱","户外防水型 (双层门)，总漏保：100A 4P 1个，分空开：25A 1P 2个，分空开：63A 3P 2个，民用插座 220V 10A 5孔 2个，五芯插座 380V 32A 2个，下进线孔M36 配防水接头 配套插头各3个 IP65 壁挂式 含4个FJ6/JTS2接线端子(一进三出 出线孔径？10mm)","","个","2.00","","","","","","电气：220KV升压站检修箱更换/"]
["11","TM2025071116054715083b8","三相水泵控制箱","0.75--3KW（含过载保护、电压、电流表，IP54） 不锈钢材质","","个","3.00","","","","","","电气：电缆沟潜水泵控制箱整改/"]
["12","TM202507111605471515061","白色护套线","国标RVV 2*2.5平方纯铜 白色外皮","","m","200.00","","","","","","电气：室内照明及插座整改/"]
["13","TM20250711160547152c777","智能电机保护器","ZDE-YP12E 75A 编号：1007531（含显示操作模块）","","套","1.00","","","","","","斗轮机电机保护器更换用/"]
["14","TM202507111605471520bdc","中间继电器","MY2N-J 8脚 220V","","个","30.00","","","","","","输煤电子间用/"]
["15","TM20250711160547153bda2","中间继电器","MY2N-J 8脚 24V DC","","个","30.00","","","","","","输煤电子间用/"]
["16","TM202507111605471548aa5","相间隔板","PB Separators H=100mm","","个","6.00","","","","","","重调机塑壳断路器配件/"]
["17","TM20250711160547155bd9e","辅助触头","AUX4Q","","个","1.00","","","","","","重调机塑壳断路器配件/"]
["18","TM202507111605471551922","漏电保护器","DZ47LE-63/C63","","个","5.00","","","","","","输煤区域检修电源箱/"]
["","合计","","","","","","","","","","",""]
["注：A、报价：无税单价（运费、装卸费出卖人承担）。"]
[" B、质量标准：国标、行业标准、企标，并注明标准号。非标产品以双方认可的图纸、协议等为准。"]
[" C、请务必填写完整、清晰，否则报价无效，修改处签章。"]
[" D、 “报价单”视为合同附件，具有法律效应。"]
[" E、付款方式：电子承兑。"]