{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["询价单"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"询价单","index":0,"n_rows":76,"n_cols":13,"rows_kept":76,"cut":false,"hidden":false,"merged":[[1,0,1,3],[1,6,1,11],[2,0,2,3],[2,6,2,11],[3,0,3,3],[3,6,3,11],[4,0,4,3],[4,6,4,11],[0,0,0,11]],"flags":["formulas_cached_only"]}
["江苏徐矿综合利用发电有限公司物资采购询（报）价单"]
["报价单位（公章或合同章）:",{"$nulls":5},"询价部门："]
["联系人:",{"$nulls":5},"联系方式："]
["传真:",{"$nulls":5},"报价截止日期："]
["供应商编码:"]
["序号","物资编码","物资名称","规格","型号","计量单位","数量","交货期","主机","无税单价（元）","总价（元）","品牌","备注"]
["1","8254110025","不锈钢活接头","DN25  304","","件","100.00","","","","","","DN25适配钢管：1寸G1(外径33MM) 适配软管：内径25MM热控"]
["2","1134210066","法兰球阀","Q41F-25P　 65mm","","只","1.00","","","","","","CF8材质，跨度220mm，配密封面垫片，介质：32号汽轮机油。密封油站用汽机"]
["3","1458500512","金属防水格兰头","M12*1.5  使用范围3-6","","只","10.00","","","","","","参数一致热控"]
["4","1568011379","液位开关","LQH-204 输出信号SPDT","","个","2.00","","","","","","供热疏水袋液位热控"]
["5","1568020615","防堵风量测量装置","YC-BM-XK","","只","1.00","","","","","","材质316L刻度流量11000，管道Φ530x5热控"]
["6","0542301727","三角带","B-1727","","根","6.00","","","","","","型号符合"]
["7","0542409000","三角带","C-9000","","根","2.00","","","","","","型号符合"]
["8","0542505334","三角带","D-5334","","根","5.00","","","","","","型号符合"]
["9","2656400054","螺母","M36*3","","只","4.00","","","","","","8级，中低压连通管志中压供热直管汽机"]
["10","2707080207","安全滑触线(4根导电带)","6mm平方/","","m","40.00","","","","","","型号符合"]
["11","2707080208","安全滑触线(4根导电带)","10mm平方/","","m","25.00","","","","","","型号符合"]
["12","2717990068","机械密封","M37G-75","","套","2.00","","","","","","双合金面密封，0米空调冷却水增压泵用。汽机"]
["13","2757290335","电机前端盖","YE3-160L-2 18.5KW","","件","1.00","","","","","","规格正确，引风机冷却风机电机"]
["14","6014010017","油漆","中灰色","","桶","2.00","","","","","","22号 25kg一桶热控"]
["15","6399000031","吊钩防脱器","5T","","个","5.00","","","","","","型号符合"]
["16","6399000032","吊钩防脱器","10T","","个","5.00","","","","","","型号符合"]
["17","6399000035","吊钩防脱器","3T","","个","5.00","","","","","","型号符合"]
["18","6407010067","非接触式无源核子料位计","CILM-04714-11702。直流24V供电，4-20mA","","个","4.00","","","","","","参数一致，安装调试热控"]
["19","6407030155","PH电极","TB556J1D15T19","","个","1.00","","","","","","PH电极热控"]
["20","6407070042","热电阻","WZP2-231 -200-450℃ L=350mm","","个","1.00","","","","","","铠装，L355MM热控"]
["21","6407090155","耐高温瓦振传感器","JK7533-09-HT-HC","","个","1.00","","","","","","安装调试，带隔热块热控"]
["22","6599000042","KAKU风扇","KA1725HA2","","个","1.00","","","","","","TSI风扇热控"]
["23","6799000055","机械密封","KQL100/220-30/2","","套","2.00","","","","","","双合金面密封，19.2米循环泵用，泵参数87m3/h，60m，2960rpm汽机"]
["24","6799000056","机械密封","KQL65/160-4/2","","套","1.00","","","","","","双合金面密封，26米补水泵用，泵参数25m3/h，32m，2960rpm汽机"]
["25","6999000900","铠装热电偶","WREK2-2306S E分度 0-800℃","","只","40.00","","","","","","φ6 E分度L440-460MM(现场测量确认)热控"]
["26","8189900100","导绳器","3T","L4201B3","个","6.00","","","","","","型号符合，3大3小"]
["27","8189900285","防爆吊钩","5T","","个","2.00","","","","","","型号符合"]
["28","6404010009","振动传感器","ZHJ-2","","只","10.00","","","","","","ZHJ-2-01-02-10-01 配电缆及航空插头热控"]
["29","6407090130","电磁流量计","DN50 介质：中水，流量范围3-35m3/h,额定压力：1.6Mpa,一体显示24V供电","","个","2.00","","","","","","HLLD-503A411AEY 通经50mm热控"]
["30","6407990001","振动传感器","VS-2H（高温型）-L04-A06-B02","","个","2.00","","","","","","参数一致热控"]
["31","6499000310","金属软管接头","DPJ一头内丝一头外丝φ25-M20*1.5","","个","100.00","","","","","","参数一致热控"]
["32","6499000311","金属软管接头","DPJ一头内丝一头外丝φ25-M25*1.5","","个","100.00","","","","","","参数一致热控"]
["33","1117450512","高强度弹垫(8级)","12mm","","十只","2.00","","","","","","#1、#4补水泵大修汽机"]
["34","1117450516","高强度弹垫(8级)","16mm","","十只","19.00","","","","","","#1、#4补水泵大修汽机"]
["35","1117450520","高强度弹垫(8级)","20mm","","十只","1.00","","","","","","#1、#4补水泵大修汽机"]
["36","1135120100","中线对夹手柄蝶阀","D71X-16   100mm","","只","7.00","","","","","","暖通系统阀门内漏，阀体球墨铸铁衬胶，阀板304不锈钢汽机"]
["37","1135120125","中线对夹手柄蝶阀","D71X-16   125mm","","只","7.00","","","","","","暖通系统阀门内漏，阀体球墨铸铁衬胶，阀板304不锈钢汽机"]
["38","141209015","行车电缆","SBH    9*1.5mm2","","m","100.00","","","","","","型号符合"]
["39","1438955960","差压开关","BH-009030-009 21-207 3450KPA 6000","","个","2.00","","","","","","定冷泵进出口差压"]
["40","0542302350","三角带","B-2350","","根","3.00","","","","","","型号符合"]
["41","1105100050","内六角螺栓","10*50mm","","十只","2.00","","","","","","全丝，8.8级，汽轮机油挡紧固螺栓汽机"]
["42","1105120050","内六角螺栓","12*50mm","","十只","1.00","","","","","","全丝，8.8级，汽轮机油挡紧固螺栓汽机"]
["43","1105160050","内六角螺栓","16*50mm","","十只","4.00","","","","","","全丝，8.8级，汽轮机油挡紧固螺栓汽机"]
["44","1105271060","不锈钢内六角螺栓","27*60mm","","十只","1.00","","","","","","A2-70,304不锈钢。汽轮机轴承箱水平面汽机"]
["45","1111120110","双头螺栓","12*110mm","","十只","1.00","","","","","","全丝，8.8级汽机"]
["46","1111160080","双头螺栓(8.8级)","16*80mm","","十只","6.00","","","","","","#1、#4补水泵大修汽机"]
["47","1114160100","高强度螺栓(8.8级)","16*100mm","","十只","7.00","","","","","","单六角头螺栓，#1、#4补水泵大修汽机"]
["48","1480301640","空调器风扇用三相异步电动机","YLS 1500W 6P  380V","","台","1.00","","","","","","含配套风机叶轮，购买前联系专业人员提供现场图片"]
["49","1114200090","高强度螺栓(8.8级)","20*90mm","","十只","1.00","","","","","","#1、#4补水泵大修汽机"]
["50","1116800012","高强度六角螺母（8级）","12mm","","十只","2.00","","","","","","普通粗牙螺母，#1、#4补水泵大修汽机"]
["51","1117450012","高强度平垫(8级)","12mm","","十只","6.00","","","","","","20只用于#1、#4补水泵大修，40只用于低压内缸隔热罩，汽机"]
["52","1117450016","高强度平垫(8级)","16mm","","十只","19.00","","","","","","#1、#4补水泵大修汽机"]
["53","1117450020","高强度平垫(8级)","20mm","","十只","1.00","","","","","","#1、#4补水泵大修汽机"]
["54","2218306315","304不锈钢包塑金属软管","黑色  φ15","","m","200.00","","","","","","参数一致热控"]
["55","1622150810","热电阻","WZPK2-336S PI100 ？6  L=300mm","","只","4.00","","","","","","风机本体热控"]
["56","1622150830","热电阻","WZPK2-236 l=200mm","","只","6.00","","","","","","参数一致热控"]
["57","1622400345","双支热电偶芯","WRNN2-436 0-950℃ L=880MM","","只","4.00","","","","","","L=850mm  φ6 K分度热控"]
["58","1622401100","热电偶","WRER2-131 E分度 L=10m φ5 活接头ZG1/4","","只","2.00","","","","","","大机本体热控"]
["59","1636200098","UPS不间断电源","UPS2000-A-3KTTS（ 3000VA/2400W 内置CSB蓄电池）","","台","3.00","","","","","","除尘输灰DCS热控"]
["60","1642050369","高清球机摄像机","DS-2DE4423IW-DE，400万2K高清，23倍变焦POE供电，360°旋转巡航","","台","2.00","","","","","","配原装支架"]
["61","1705630023","螺丝刀批头","SD-2310","","套","1.00","","","","","","型号一致热控"]
["62","1708310126","电动扳手","博士GDS18V-400","","台","1.00","","","","","","正品质保，转换头，批头热控"]
["63","1939011288","气管外螺纹快拧直接头","1/4*φ8","","只","100.00","","","","","","304 ZG1/4-8mm热控"]
["64","1939070802","气动接头","PC外螺纹直通接头 PC8-02 气管直径8mm，螺纹直径1/4\"","","只","100.00","","","","","","参数一致热控"]
["","合计","","","","","","","","","","",""]
["注：A、报价：无税单价（运费、装卸费出卖人承担）。"]
[" B、质量标准：国标、行业标准、企标，并注明标准号。非标产品以双方认可的图纸、协议等为准。"]
[" C、请务必填写完整、清晰，否则报价无效，修改处签章。"]
[" D、 “报价单”视为合同附件，具有法律效应。"]
[" E、付款方式：电子承兑。"]