{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["询价单"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"询价单","index":0,"n_rows":57,"n_cols":13,"rows_kept":57,"cut":false,"hidden":false,"merged":[[1,0,1,3],[1,6,1,11],[2,0,2,3],[2,6,2,11],[3,0,3,3],[3,6,3,11],[4,0,4,3],[4,6,4,11],[0,0,0,11]],"flags":["formulas_cached_only"]}
["江苏华美热电有限公司物资采购询（报）价单"]
["报价单位（公章或合同章）:",{"$nulls":5},"询价部门："]
["联系人:",{"$nulls":5},"联系方式："]
["传真:",{"$nulls":5},"报价截止日期："]
["供应商编码:"]
["序号","物资编码","物资名称","规格","型号","计量单位","数量","交货期","主机","无税单价（元）","总价（元）","品牌","备注"]
["1","TM20251016150002657fdf9","塑料薄膜","宽1m","","m","200.00","","","","","","材质:线型低密度聚乙烯"]
["2","TM2025101615000265965a5","警示牌","400*600*2mm  铝板等离子切割打孔反光贴","","块","20.00","","","","","","按400*300大小裁成2半,内容见样图，内容字样耐150°高温不变色"]
["3","TM202510161500026604539","铁芯万向轮","8寸；轮子直径20cm  轮子宽5cm 安装高度24.5厘米","","个","6.00","","","","","",""]
["4","TM202510161500026613e1f","粘鼠板","22*17cm","","个","30.00","","","","","",""]
["5","TM20251016150002662d713","长统胶靴","矿用","","双","5.00","","","","","","40码1双，43码1双，44码3双"]
["6","TM202510161500026631308","分体式雨衣","PVC牛津布标准雨帽上 衣裤子带反光条","","套","8.00","","","","","","XL2套、XXL4套、XXXL2套"]
["7","TM20251016150002664217f","堵漏王","5kg/袋","","kg","50.00","","","","","",""]
["8","TM20251016150002664a4bf","螺栓松动润滑防锈剂","450ml/罐","","罐","24.00","","","","","","康尔达"]
["9","TM202510161500026653a2e","金属软管管接","Ф25镀锌","","套","20.00","","","","","",""]
["10","TM202510161500026665d63","柜门锁","AB301\n锌合金\n长*宽:147*33","","把","5.00","","","","","",""]
["11","TM20251016150002667c21e","柜门锁","MS818-1","","个","10.00","","","","","",""]
["12","TM20251016150002667182d","防火锁","CB-SIS","","套","8.00","","","","","","可见样品"]
["13","TM2025101615000266852fb","弹跳式把手锁","AB303-1","","把","10.00","","","","","",""]
["14","TM2025101615000266980c0","三联鹅颈水龙头","白色，鹅颈管高度：500~600mm，主体材质：黄铜，陶瓷阀芯，配生料带一卷，1米金属编织软管一根","","个","1.00","","","","","",""]
["15","TM20251016150002670f106","玻璃胶","300ML/瓶 (透明)","","瓶","5.00","","","","","","中性"]
["16","TM2025101615000267045cb","电动三轮车调速转把","ZS800DQZH/宗申","","件","1.00","","","","","",""]
["17","TM202510161500026712453","塑料水桶","10kg","","只","4.00","","","","","",""]
["18","TM202510161500026717d9c","警戒绳","带三角旗","","m","1000.00","","","","","","2.5mm粗圆绳"]
["19","TM202510161500026729c07","棉布","卫生清扫","","kg","60.00","","","","","",""]
["20","TM2025101615000267383f2","鹿皮抹布","43*32cm","","张","3.00","","","","","",""]
["21","TM2025101615000267320ad","LED头灯","世达90902，锂电款，带充电器，可磁吸，可头戴","","个","2.00","","","","","",""]
["22","TM2025101615000267415b2","微型头灯","额定功率：1W,额定电压：3.7V，容量2.2Ah,连续放电：强光≥8h,工作光≥16h,防护等级IP66,外形尺寸：97*50*63，重量95g，弹性帽带｛含4个帽勾｝","","个","6.00","","","","","",""]
["23","TM20251016150002675e239","防爆手提灯","LED(60W)  强光≥4h 工作光≥8h 尺寸：260×200×184mm 重量：3.8kg  防爆等级IP66 配光角度：匀光150°","","个","2.00","","","","","",""]
["24","TM20251016150002675f9cb","记号笔","双头 6824","","支","2.00","","","","","",""]
["25","TM20251016150002676d9c9","油性记号笔","黑色","","支","20.00","","","","","",""]
["26","TM202510161500026779b26","油性记号笔","白色","","只","20.00","","","","","",""]
["27","TM20251016150002677aa9a","油漆笔","白色","","只","36.00","","","","","","中柏"]
["28","TM20251016150002678a475","油漆笔","黑色","","支","24.00","","","","","","中柏"]
["29","TM20251016150002679d437","油漆笔","红色","","支","24.00","","","","","","中柏"]
["30","TM20251016150002679456e","石笔","110*12*4","","支","60.00","","","","","",""]
["31","TM20251016150002680a79f","白板笔","","","支","2.00","","","","","",""]
["32","TM202510161500026819128","白板磁铁","30mm","","个","10.00","","","","","",""]
["33","TM20251016150002681701e","羊毛刷","50mm 2\"","","把","10.00","","","","","",""]
["34","TM20251016150002682dbf5","羊毛刷","75mm 3\"","","把","10.00","","","","","",""]
["35","TM202510161500026823c67","LED照明灯","光源：LED(60W) 强光续航≥4h，工作光续航≥8h 尺寸：260*200*134mm（聚光） 防护等级IP66 配光角度30° 带支架可调节方向","","个","2.00","","","","","","品牌：尚为、紫光、海洋王三选一"]
["36","TM202510161500026833f93","明线盒","86HM33Ⅱ","","只","10.00","","","","","",""]
["37","TM20251016150002683f3bf","电磁阀","SCG551A001MS,230/50  ASCO","","个","5.00","","","","","",""]
["38","TM202510161500026845130","空气开关","IC65N  D25A","","个","2.00","","","","","","3P"]
["39","TM20251016150002685a1bf","LED照明灯","220V 200W","","盏","2.00","","","","","","铝合金外壳，带散热片及支架"]
["40","TM20251016150002685b78b","独立支架LED照明灯","LED光源,额度功率60W,14.8V,133Wh,循环寿命≥1500次充放电，强光≥4h,工作光≥8h,充电时间≤6h，防护等级IP66,防腐等级WF2,重量3.8kg,大小尺寸260*200*134（聚光），材质，铝合金","","只","2.00","","","","","","尚为，海洋王，创硕三选一"]
["41","TM20251016150002686eb0f","触摸屏","MT8070iH 3WV","","台","1.00","","","","","",""]
["42","TM20251016150002686e373","操作台座椅","100MM气压棒,340MM尼龙椅脚，60MM滑轮","","组","1.00","","","","","",""]
["43","TM202510161500026877a22","DPT-8清洗剂（着色）","净重283g/500mL喷雾罐装","","瓶","800.00","","","","","","新美达"]
["44","TM202510161500026884aec","DPT-8渗透剂（着色）","净重278g/500mL喷雾罐装","","瓶","172.00","","","","","","新美达"]
["45","TM202510161500026887e99","DPT-8显像剂（着色）","净重304g/500mL喷雾罐装","","瓶","252.00","","","","","","新美达"]
["","合计","","","","","","","","","","",""]
["注：A、报价：无税单价（运费、装卸费出卖人承担）。"]
[" B、质量标准：国标、行业标准、企标，并注明标准号。非标产品以双方认可的图纸、协议等为准。"]
[" C、请务必填写完整、清晰，否则报价无效，修改处签章。"]
[" D、 “报价单”视为合同附件，具有法律效应。"]
[" E、付款方式：电子承兑。"]