{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["询价单"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"询价单","index":0,"n_rows":29,"n_cols":13,"rows_kept":29,"cut":false,"hidden":false,"merged":[[1,0,1,3],[1,6,1,11],[2,0,2,3],[2,6,2,11],[3,0,3,3],[3,6,3,11],[4,0,4,3],[4,6,4,11],[0,0,0,11]],"flags":["formulas_cached_only"]}
["江苏省矿业工程集团有限公司安装分公司物资采购询（报）价单"]
["报价单位（公章或合同章）:",{"$nulls":5},"询价部门："]
["联系人:",{"$nulls":5},"联系方式："]
["传真:",{"$nulls":5},"报价截止日期："]
["供应商编码:"]
["序号","物资编码","物资名称","规格","型号","计量单位","数量","交货期","主机","含税单价（元）","总价（元）","品牌","备注"]
["1","TM202510212205372268770","球墨铸铁管","球墨铸铁管DN300球管压力等级C30，球墨铸铁管防腐采用内衬高铝水泥，外喷涂锌层及红色沥青漆。球墨铸铁管外防腐采用锌+铁红色环氧漆。","球墨铸铁管DN300球管压力等级C30，球墨铸铁管防腐采用内衬高铝水泥，外喷涂锌层及红色沥青漆。球墨铸铁管外防腐采用锌+铁红色环氧漆。","m","103.00","","","","","","按项目部要求规格型号及时送货，如是定制材料请联系项目部"]
["2","TM20251021220537228a409","球墨铸铁管","球墨铸铁管DN400球管压力等级C30，球墨铸铁管防腐采用内衬高铝水泥，外喷涂锌层及红色沥青漆。球墨铸铁管外防腐采用锌+铁红色环氧漆","球墨铸铁管DN400球管压力等级C30，球墨铸铁管防腐采用内衬高铝水泥，外喷涂锌层及红色沥青漆。球墨铸铁管外防腐采用锌+铁红色环氧漆","m","4.00","","","","","","按项目部要求规格型号及时送货，如是定制材料请联系项目部"]
["3","TM20251021220537229685c","球墨铸铁管","球墨铸铁管DN300球管压力等级C30，球墨铸铁管防腐采用内衬高铝水泥，外喷涂锌层及红色沥青漆。球墨铸铁管外防腐采用锌+铁红色环氧漆","球墨铸铁管DN300球管压力等级C30，球墨铸铁管防腐采用内衬高铝水泥，外喷涂锌层及红色沥青漆。球墨铸铁管外防腐采用锌+铁红色环氧漆","m","90.00","","","","","","按项目部要求规格型号及时送货，如是定制材料请联系项目部"]
["4","TM202510212205372308c73","塑料管","1、材质及规格：DN80软管（耐磨压）\n2、其他详见图纸","1、材质及规格：DN80软管（耐磨压）\n2、其他详见图纸","m","60.00","","","","","","按项目部要求规格型号及时送货，如是定制材料请联系项目部"]
["5","TM202510212205372310692","聚氨酯直埋保温无缝钢管","1、规格、压力等级：钢管D273X6\n2、其他详见图纸","1、规格、压力等级：钢管D273X6\n2、其他详见图纸","m","4.30","","","","","","按项目部要求规格型号及时送货，如是定制材料请联系项目部"]
["6","TM2025102122053723333d0","聚氨酯直埋保温无缝钢管","1、规格、压力等级：钢管D325*7\n2、其他详见图纸","1、规格、压力等级：钢管D325*7\n2、其他详见图纸","m","3.30","","","","","","按项目部要求规格型号及时送货，如是定制材料请联系项目部"]
["7","TM20251021220537234db4e","高清网络摄像机","400W像素,1080P,0.1LUX低照度日夜转换,22倍变焦,云台控制可选,配供24V电源适配器,室内安装防护等级IP54,室外安装防护等级IP67","400W像素,1080P,0.1LUX低照度日夜转换,22倍变焦,云台控制可选,配供24V电源适配器,室内安装防护等级IP54,室外安装防护等级IP67","台","5.00","","","","","","按项目部要求规格型号及时送货，如是定制材料请联系项目部"]
["8","TM20251021220537235ea1f","安装支架","1、名称：摄像机立杆（基础支架落地基础）\n2、规格：杆高4.0m，不锈钢304，含底座、基础、接闪器等 \n3、其他未注明事项详见图纸要求","1、名称：摄像机立杆（基础支架落地基础）\n2、规格：杆高4.0m，不锈钢304，含底座、基础、接闪器等 \n3、其他未注明事项详见图纸要求","个","5.00","","","","","","按项目部要求规格型号及时送货，如是定制材料请联系项目部"]
["9","TM202510212205372361807","分体式高清视频终端","1、名称：视频终端箱\n2、类别：箱内设置开关电源、8口POE交换机、光纤终端盒等\n3、其他未注明事项详见图纸要求","1、名称：视频终端箱\n2、类别：箱内设置开关电源、8口POE交换机、光纤终端盒等\n3、其他未注明事项详见图纸要求","套","2.00","","","","","","按项目部要求规格型号及时送货，如是定制材料请联系项目部"]
["10","TM20251021220537236f42f","防雷器","1、名称：电源信号二合一防雷器\n2、其他未注明事项详见图纸要求","1、名称：电源信号二合一防雷器\n2、其他未注明事项详见图纸要求","件","2.00","","","","","","按项目部要求规格型号及时送货，如是定制材料请联系项目部"]
["11","TM2025102122053723725e8","磁盘阵列","1、名称：监控磁盘阵列\n2、规格：不少于24个硬盘位,单盘最大支持8T\n3、其他未注明事项详见图纸要求","1、名称：监控磁盘阵列\n2、规格：不少于24个硬盘位,单盘最大支持8T\n3、其他未注明事项详见图纸要求","台","1.00","","","","","","按项目部要求规格型号及时送货，如是定制材料请联系项目部"]
["12","TM20251021220537238807f","NAS用存储硬盘","1、名称：监控专用存储硬盘\n2、规格：8T\n3、其他未注明事项详见图纸要求","1、名称：监控专用存储硬盘\n2、规格：8T\n3、其他未注明事项详见图纸要求","块","3.00","","","","","","按项目部要求规格型号及时送货，如是定制材料请联系项目部"]
["13","TM20251021220537239f268","电力电缆","型号：YJV-0.6/1kV-3×4","型号：YJV-0.6/1kV-3×4","m","300.00","","","","","","按项目部要求规格型号及时送货，如是定制材料请联系项目部"]
["14","TM20251021220537239e181","单模光纤","四芯单模光纤","四芯单模光纤","m","300.00","","","","","","按项目部要求规格型号及时送货，如是定制材料请联系项目部"]
["15","TM2025102122053724035d8","超五类室外双层阻水防水网线","室外防水型超五类网线","室外防水型超五类网线","m","150.00","","","","","","按项目部要求规格型号及时送货，如是定制材料请联系项目部"]
["16","TM20251021220537241993c","电源线","RW-2*2.5","RW-2*2.5","m","150.00","","","","","","按项目部要求规格型号及时送货，如是定制材料请联系项目部"]
["17","TM20251021220537242a9f4","PE管","PE32","PE32","m","500.00","","","","","","按项目部要求规格型号及时送货，如是定制材料请联系项目部"]
["","合计","","","","","","","","","","",""]
["注：A、报价：无税单价（运费、装卸费出卖人承担）。"]
[" B、质量标准：国标、行业标准、企标，并注明标准号。非标产品以双方认可的图纸、协议等为准。"]
[" C、请务必填写完整、清晰，否则报价无效，修改处签章。"]
[" D、 “报价单”视为合同附件，具有法律效应。"]
[" E、付款方式：电子承兑。"]