{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["询价单"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"询价单","index":0,"n_rows":26,"n_cols":13,"rows_kept":26,"cut":false,"hidden":false,"merged":[[1,0,1,3],[1,6,1,11],[2,0,2,3],[2,6,2,11],[3,0,3,3],[3,6,3,11],[4,0,4,3],[4,6,4,11],[0,0,0,11]],"flags":["formulas_cached_only"]}
["陕西长青能源化工有限公司物资采购询（报）价单"]
["报价单位（公章或合同章）:",{"$nulls":5},"询价部门："]
["联系人:",{"$nulls":5},"联系方式："]
["传真:",{"$nulls":5},"报价截止日期："]
["供应商编码:"]
["序号","物资编码","物资名称","规格","型号","计量单位","数量","交货期","主机","含税单价（元）","总价（元）","品牌","备注"]
["1","TM2025051416122789391d5","不锈钢六角外丝直通","DN20  304","","件","5.00","","","","","","动力仓泵压力表进气管接头检修"]
["2","TM2025051416122789561c3","防爆声光报警器","AEC2323 不锈钢壳体 红色PC灯罩 工作电压：DC24V±6V 工作电流：＜100mA  光强：2400±200mcd 声音强度：≥85dBF防爆标志：ExdibllCT6 防护等级：IP65 出线孔连接螺纹：G3/4管螺纹（外）配套安可信气体报警器用","","台","3.00","","","","","","气体报警器维护标定使用"]
["3","TM2025051416122789632ab","卡套式弯通接头","1/4NPT转φ12，材质：304   直角","","只","4.00","","","","","","气化炉锁斗系统阀门检修"]
["4","TM20250514161227897feb7","卡套式弯通接头","3/8NPT转φ10，材质：304   直角","","只","4.00","","","","","","气化炉锁斗系统阀门检修"]
["5","TM2025051416122789881c1","卡套式弯通接头","3/8NPT转φ12，材质：304   直角","","只","4.00","","","","","","气化炉锁斗系统阀门检修"]
["6","TM20250514161227898d8af","宝塔外丝接头","DN20，材质：304","","个","3.00","","","","","","动力仓泵压力表进气管接头检修"]
["7","TM20250514161227899dfe2","24V电源模块","S-25-24 输入：220V AC，输出：24V 1A","","件","1.00","","","","","","火炬改造工程"]
["8","TM20250514161227900becb","仪表风线管","软风线    Φ10   材质：聚氨酯（PU)","","m","30.00","","","","","","蓝色，动力布袋除尘器提升阀气源管更换用"]
["9","TM202505141612279014e8b","仪表风线管","软风线    Φ10   材质：聚氨酯（PU)","","m","30.00","","","","","","气化炉锁斗系统阀门检修"]
["10","TM2025051416122790288cc","回讯器","ITS-100,内含2*SPDT开关，输出触点：16A 250V","","台","2.00","","","","","","供水装置检修"]
["11","TM20250514161227903afa0","宝塔消音器","DN32 外丝，304","","个","4.00","","","","","","气化炉锁斗系统阀门检修"]
["12","TM20250514161227903e410","气动三联件","GF400-10+GR400-10+GL400-10","亚德客/SMC","个","1.00","","","","","","动力硫酸铵包装机气源管路过滤减压阀检修，亚德客/SMC"]
["13","TM2025051416122790424fc","密封组件","CA2-100Z-PS  SMC","SMC","套","8.00","","","","","","动力布袋除尘器提升阀检修，SMC"]
["14","TM20250514161227905a9c6","热缩套管","φ50mm   收缩比2：1  1kv, 黑色","","m","2.40","","","","","","K2301B高压电机变更低压电机改造"]
["","合计","","","","","","","","","","",""]
["注：A、报价：无税单价（运费、装卸费出卖人承担）。"]
[" B、质量标准：国标、行业标准、企标，并注明标准号。非标产品以双方认可的图纸、协议等为准。"]
[" C、请务必填写完整、清晰，否则报价无效，修改处签章。"]
[" D、 “报价单”视为合同附件，具有法律效应。"]
[" E、付款方式：电子承兑。"]