{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["询价单"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"询价单","index":0,"n_rows":34,"n_cols":13,"rows_kept":34,"cut":false,"hidden":false,"merged":[[1,0,1,3],[1,6,1,11],[2,0,2,3],[2,6,2,11],[3,0,3,3],[3,6,3,11],[4,0,4,3],[4,6,4,11],[0,0,0,11]],"flags":["formulas_cached_only"]}
["江苏新美建筑工程有限公司物资采购询（报）价单"]
["报价单位（公章或合同章）:",{"$nulls":5},"询价部门："]
["联系人:",{"$nulls":5},"联系方式："]
["传真:",{"$nulls":5},"报价截止日期："]
["供应商编码:"]
["序号","物资编码","物资名称","规格","型号","计量单位","数量","交货期","主机","含税单价（元）","总价（元）","品牌","备注"]
["1","TM202307211747240881cad","两台激光切割机基础","","","","1.00","","","","","",""]
["2","TM202307211747240901a88","钢筋混凝土构件拆除\n1、构件名称：混凝土地面\n2、拆除构件的厚度或规格尺寸：厚20-30cm\n3、垃圾外运","1","1","m2","77.00","","","","","","1、构件名称：混凝土地面2、拆除构件的厚度或规格尺寸：厚20-30cm3、垃圾外运"]
["3","TM20230721174724091e815","混凝土构件拆除\n1.构件名称：钢筋混凝土设备基础拆除","1","1","m3","64.80","","","","","","1.构件名称：钢筋混凝土设备基础拆除"]
["4","TM20230721174724092c67b","挖一般土方\n1、土壤类别：根据现场勘查自行考虑\n2、挖土深度：0.7m","1","1","m3","15.40","","","","","","1、土壤类别：根据现场勘查自行考虑2、挖土深度：0.7m"]
["5","TM2023072117472409367dc","余方弃置\n1、运距：自行考虑（部分内倒）","1","1","m3","87.90","","","","","","1、运距：自行考虑（部分内倒）"]
["6","TM202307211747240944a9b","带形基础\n1、混凝土强度等级：C30细石砼基础","1","1","m3","30.80","","","","","","1、混凝土强度等级：C30细石砼基础（混凝土甲供）2、模板综合考虑"]
["7","TM20230721174724094b2d4","预埋铁件\n1、钢材种类：预埋钢板（钢板甲供）","1","1","t","1.59","","","","","","1、钢材种类：预埋钢板（钢板甲供）"]
["8","TM202307211747240972ab6","现浇构件钢筋\n1、钢筋种类、规格：Φ12","1","1","t","1.19","","","","","","1、钢筋种类、规格：Φ12"]
["9","TM2023072117472409739ef","现浇构件钢筋\n1、钢筋种类、规格：Φ16","1","1","t","0.70","","","","","","1、钢筋种类、规格：Φ16"]
["10","TM2023072117472409872b2","一般抹灰","1","1","m2","6.00","","","","","","抹灰"]
["11","TM20230721174724099b04e","垫层\n新做C30砼底50厚","1","1","m3","0.75","","","","","","新做C30砼底50厚（砼甲供）"]
["12","TM20230721174724100dd9c","地坪","","","","1.00","","","","","",""]
["13","TM202307211747241014dd6","混凝土构件拆除\n切割机切砼边斜坡","1","1","m","50.00","","","","","","切割机切砼边斜坡"]
["14","TM20230721174724101e128","打磨地面\n地面打磨多遍，满足油漆","1","1","m2","1200.00","","","","","","地面打磨多遍，满足油漆（生产设备保护，打磨施工吸尘器收尘等自行考虑）"]
["15","TM20230721174724102c005","水泥砂浆楼地面\n原地坪面修补","1","1","m2","500.00","","","","","","原地坪面修补、找平，满足油漆"]
["16","TM20230721174724103de33","余方弃置\n垃圾外运","1","1","m3","10.00","","","","","","1.垃圾外运2.运距综合考虑"]
["17","TM202307211747241034dd2","危废库平台","","","","1.00","","","","","",""]
["18","TM20230721174724104946b","实心砖墙\n砌240砖墙40㎡、抹灰、粉刷腻子二遍、乳胶漆一遍","1","1","m3","9.60","","","","","","砌240砖墙40㎡、抹灰、粉刷腻子二遍、乳胶漆一遍"]
["19","TM2023072117472410558b7","回填方","1","1","m3","70.00","","","","","","回填土渣土砂石分层压实"]
["20","TM202307211747241057b9d","现浇混凝土人行道及进口坡","1","1","m2","95.20","","","","","","20cm厚砼坡道路面（砼甲供）2.模板综合考虑"]
["21","TM20230721174724106723f","砖砌体拆除\n拆除单砖墙","1","1","m3","3.60","","","","","","拆除单砖墙"]
["22","TM20230721174724107a171","余方弃置\n垃圾外运","1","1","m3","3.60","","","","","","1.垃圾外运（部分内倒），2.运距综合考虑"]
["","合计","","","","","","","","","","",""]
["注：A、报价：无税单价（运费、装卸费出卖人承担）。"]
[" B、质量标准：国标、行业标准、企标，并注明标准号。非标产品以双方认可的图纸、协议等为准。"]
[" C、请务必填写完整、清晰，否则报价无效，修改处签章。"]
[" D、 “报价单”视为合同附件，具有法律效应。"]
[" E、付款方式：电子承兑。"]