{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["询价单"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"询价单","index":0,"n_rows":23,"n_cols":13,"rows_kept":23,"cut":false,"hidden":false,"merged":[[1,0,1,3],[1,6,1,11],[2,0,2,3],[2,6,2,11],[3,0,3,3],[3,6,3,11],[4,0,4,3],[4,6,4,11],[0,0,0,11]],"flags":["formulas_cached_only"]}
["陕西长青能源化工有限公司物资采购询（报）价单"]
["报价单位（公章或合同章）:",{"$nulls":5},"询价部门："]
["联系人:",{"$nulls":5},"联系方式："]
["传真:",{"$nulls":5},"报价截止日期："]
["供应商编码:"]
["序号","物资编码","物资名称","规格","型号","计量单位","数量","交货期","主机","含税单价（元）","总价（元）","品牌","备注"]
["1","TM2025080611480823290c2","旋转密封阀","QH3.00","棒磨机气动离合器QL1000-300*2","个","1.00","","","","","","H1201A/B现场用泰州东方生产"]
["2","TM202508061148082348676","旋转密封阀","XZJT-25A  棒磨机H1201C","","件","1.00","","","","","","H1201C,现场用格瑞德品牌"]
["3","TM20250806114808235ccc2","闸阀","Z41H-16C  RF  DN100 WCB/13Cr","--煤化工专用","台","1.00","","","","","","污水大事故池旁管线"]
["4","TM20250806114808236783a","内螺纹球阀","Q11F -10P  DN15   PN1.0   304","","台","3.00","","","","","","机泵压力表根部阀"]
["5","TM20250806114808236e12e","球阀","Q41F46-10C  DN25  RF WCB/F46","全衬氟（包含阀芯）","台","3.00","","","","","","硫回收机泵导淋维护"]
["6","TM20250806114808237be0c","球阀","Q41F46-16P  DN40 PN1.6Mpa  RF   316L/F46，介质：硫酸铵溶液 温度：70度。","","台","3.00","","","","","","硫回收机泵导淋维护"]
["7","TM20250806114808238b647","三片式球阀","Q61F-16C DN20 WCB","","件","1.00","","","","","","循环水硫酸投加管线"]
["8","TM20250806114808239611c","三片式球阀","Q61F-16C DN50 WCB","","件","2.00","","","","","","循环水硫酸投加管线"]
["9","TM20250806114808240cefc","对夹式电动衬胶蝶阀","D971X-16C    DN250  WCB电动执行机构要带固定的手轮，可以力矩调节，公称压力下无泄漏，带密封性试验报告，电动执行机构与阀杆为正方体形连接.。","","台","1.00","","","","","","供水装置用/参考厂家：盖米，依博罗，博雷"]
["10","TM20250806114808241a7a2","对夹式衬胶气动蝶阀","DN200   PS:10.0bar   TS:-10℃/+120℃  阀体材质：GGG40（球磨铸铁），带环氧树脂涂层（厚度250微米）；阀板材质316；衬胶及密封材质：EPDM(三元乙丙橡胶；气缸：齿轮齿条双作用，铝合金材质，带直径为6mm的快插接头，带回讯器，防护等级：IP67.","","台","1.00","","","","","","供水装置用"]
["11","TM2025080611480824187cb","内螺纹截止阀","J11W-16  DN20  PN1.6Mpa  304，阀体长度55mm","","个","2.00","","","","","","P2101AB"]
["","合计","","","","","","","","","","",""]
["注：A、报价：无税单价（运费、装卸费出卖人承担）。"]
[" B、质量标准：国标、行业标准、企标，并注明标准号。非标产品以双方认可的图纸、协议等为准。"]
[" C、请务必填写完整、清晰，否则报价无效，修改处签章。"]
[" D、 “报价单”视为合同附件，具有法律效应。"]
[" E、付款方式：电子承兑。"]