{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["询价单"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"询价单","index":0,"n_rows":30,"n_cols":13,"rows_kept":30,"cut":false,"hidden":false,"merged":[[1,0,1,3],[1,6,1,11],[2,0,2,3],[2,6,2,11],[3,0,3,3],[3,6,3,11],[4,0,4,3],[4,6,4,11],[0,0,0,11]],"flags":["formulas_cached_only"]}
["江苏徐矿能源股份有限公司物资供销分公司物资采购询（报）价单"]
["报价单位（公章或合同章）:",{"$nulls":5},"询价部门："]
["联系人:",{"$nulls":5},"联系方式："]
["传真:",{"$nulls":5},"报价截止日期："]
["供应商编码:"]
["序号","物资编码","物资名称","规格","型号","计量单位","数量","交货期","主机","含税单价（元）","总价（元）","品牌","备注"]
["1","6014010006","气化板","150×300","","只","14.00","","","","","","下述配件均直发阿克苏电厂，150*300mm（气化板、气化槽一体式）透气孔：41um 透气度：3.6 透气能力：0.73 气孔率：28 抗压强度：＞35Mpa 抗折强度：＞15Mpa 气化板材质：SiC ，电场气化板、粗细灰库更换"]
["2","6014070026","补气环","DN150","","个","50.00","","","","","","DN150 材质：NM400，电除尘二三四电场使用"]
["3","6016050019","螺旋电缆","Ik系列吹灰器配套使用，总长10m 4芯2.5平方左旋","","根","2.00","","","","","","Ik系列吹灰器配套使用，总长10m 4芯2.5平方左旋 戴蒙德 耐温120℃以上"]
["4","6016050020","螺旋电缆","Ik系列吹灰器配套使用，总长10m 4芯2.5平方右旋","","根","2.00","","","","","","Ik系列吹灰器配套使用，总长10m 4芯2.5平方右旋 戴蒙德 耐温120℃以上"]
["5","6114010029","主油箱换热胶条","GX-100X197","","条","220.00","","","","","","GX-100X197，主油箱板换使用"]
["6","6114010044","主油箱板换换热片","主油箱冷却器型号\nGX—100X197  \n材质TP316L","","片","30.00","","","","","","主油箱冷却器型号：GX—100X197；材质TP316L；重要辅机备件：传特板式换热器（北京）有限公司，主油箱板换使用"]
["7","6114030014","滤芯","HC8314FKT16H","","个","4.00","","","","","","HC8314FKT16H 原品牌：PALL，密封油站使用"]
["8","6403010090","主控板","澳托克IKTM","","块","1.00","","","","","","上海澳托克IKTM配套使用"]
["9","6403010090","主控板","澳托克IKTM","","块","1.00","","","","","","上海澳托克IKTM配套使用"]
["10","6403010157","IQ三代绝对编码器","MOD 77498G","","块","1.00","","","","","","IQ三代 MOD77498G"]
["11","6403010178","电源板","配套RAⅢ130AF16B温州瑞基使用","","块","1.00","","","","","","配套RAⅢ130AF16B温州瑞基使用"]
["12","6403010179","电源板","上海澳托克IK25","","块","1.00","","","","","","上海澳托克IK25配套使用"]
["13","6405010020","电磁阀","4WE-6-DOF/E-W240-20","","个","2.00","","","","","","热控材料：磨煤机加载油站换向阀、升降磨辊使用"]
["14","6405010052","直动式电磁提升电磁阀","NORGREN 2401103（带线圈）电磁 阀","","块","2.00","","","","","","2401103（带线圈和方形底座）电磁阀 NORGREN"]
["15","6499000269","双杯过滤器减压阀","AFR2000-AL2000","","个","4.00","","","","","","双杯过滤器减压阀（过滤减压阀+油雾器）"]
["16","6507070036","6KV开关推进机构","开关型号：VB2   1250A","","套","2.00","","","","","","配套长城开关型号：VB2 1250A"]
["17","6507070037","6KV开关推进机构","开关型号：JCZR16-7.2J/D  160A","","套","2.00","","","","","","配套长城开关型号：JCZR16-7.2J/D 160A"]
["18","6604030003","针型阀","J23W-320P 304 DN6 T≤540°C","","个","4.00","","","","","","不锈钢DN06 J23W-320P 316SS材质 工作温度耐温540℃"]
["","合计","","","","","","","","","","",""]
["注：A、报价：无税单价（运费、装卸费出卖人承担）。"]
[" B、质量标准：国标、行业标准、企标，并注明标准号。非标产品以双方认可的图纸、协议等为准。"]
[" C、请务必填写完整、清晰，否则报价无效，修改处签章。"]
[" D、 “报价单”视为合同附件，具有法律效应。"]
[" E、付款方式：电子承兑。"]