{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["询价单"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"询价单","index":0,"n_rows":26,"n_cols":13,"rows_kept":26,"cut":false,"hidden":false,"merged":[[1,0,1,3],[1,6,1,11],[2,0,2,3],[2,6,2,11],[3,0,3,3],[3,6,3,11],[4,0,4,3],[4,6,4,11],[0,0,0,11]],"flags":["formulas_cached_only"]}
["江苏徐矿能源股份有限公司物资供销分公司物资采购询（报）价单"]
["报价单位（公章或合同章）:",{"$nulls":5},"询价部门："]
["联系人:",{"$nulls":5},"联系方式："]
["传真:",{"$nulls":5},"报价截止日期："]
["供应商编码:"]
["序号","物资编码","物资名称","规格","型号","计量单位","数量","交货期","主机","含税单价（元）","总价（元）","品牌","备注"]
["1","8222120202","闸阀","Z41H-25C DN20 RF A105/13Cr，介质杂醇，温度≤425℃。","","台","2.00","","","","","","直发长青能化，报价包含运费，卸货费"]
["2","8222210202","闸阀","Z41Y-600LBC   DN20  RF   A105/STL，介质粗甲醇，温度≤425℃。","","台","2.00","","","","","","直发长青能化，报价包含运费，卸货费"]
["3","8222218003","闸阀","Z41Y-150LBP  DN25   RF  CF8/STL，介质脱盐水，常温。","","台","1.00","","","","","","直发长青能化，报价包含运费，卸货费"]
["4","8222628803","焊接闸阀","Z61H-800LBP  DN25   BW  304/CF8，介质：污水；适用温度≤200℃。","","台","2.00","","","","","","直发长青能化，报价包含运费，卸货费"]
["5","8222992003","衬氟闸阀","Z41F46 DN25-150LB  阀体 阀盖 阀瓣316 内衬F46 阀杆 不锈钢 填料F4，介质：含氨废水 温度90度。","","台","2.00","","","","","","美标法兰磅级，国标的法兰长度（两法兰密封面之间的距离）；推荐品牌：中国上正阀门/精工阀门/五洲阀门/良工阀门/立信阀门/无锡美瑞克；直发长青能化，报价包含运费，卸货费"]
["6","8222992006","衬氟闸阀","Z41F46 DN50-150LB  阀体 阀盖 阀瓣316 内衬F46 阀杆 不锈钢 填料F4 长度约178mm，介质：含氨废水 温度90度。","","台","7.00","","","","","","美标法兰磅级，国标的法兰长度（两法兰密封面之间的距离）；推荐品牌：中国上正阀门/精工阀门/五洲阀门/良工阀门/立信阀门/无锡美瑞克；直发长青能化，报价包含运费，卸货费"]
["7","8222992009","衬氟闸阀","Z41F46 DN80-150LB  阀体 阀盖 阀瓣316 内衬F46 阀杆 不锈钢 填料F4,长度约=204mm，介质：含氨废水 温度90度。","","台","2.00","","","","","","美标法兰磅级，国标的法兰长度（两法兰密封面之间的距离）；推荐品牌：中国上正阀门/精工阀门/五洲阀门/良工阀门/立信阀门/无锡美瑞克；直发长青能化，报价包含运费，卸货费"]
["8","8222992010","衬氟闸阀","Z41F46 DN100-150LB  阀体 阀盖 阀瓣316 内衬F46 阀杆 不锈钢 填料F4，介质：含氨废水 温度90度。","","台","4.00","","","","","","美标法兰磅级，国标的法兰长度（两法兰密封面之间的距离）；推荐品牌：中国上正阀门/精工阀门/五洲阀门/良工阀门/立信阀门/无锡美瑞克；直发长青能化，报价包含运费，卸货费"]
["9","8223530009","陶瓷球阀","Q347C-150LB DN80 RF  WCB/STL，介质：黑水（含渣） 温度60度。","","台","1.00","","","","","","材质：氧化锆；直发长青能化，报价包含运费，卸货费"]
["10","8225240203","截止阀","J41Y-600LBC   DN25  RF  A105/STL，介质锅炉给水，温度≤425℃。","","台","1.00","","","","","","直发长青能化，报价包含运费，卸货费"]
["11","8225344203","截止阀","J41F-25P DN25 FM  CF8，适用温度≤200℃。","注：适用于介质为氨、氨液 （属专用阀门）","台","1.00","","","","","","推荐品牌：中国上正阀门/精工阀门/五洲阀门/良工阀门/立信阀门/无锡美瑞克；直发长青能化，报价包含运费，卸货费"]
["12","8225344203","截止阀","J41F-25P DN25 FM  CF8，适用温度≤200℃。","注：适用于介质为氨、氨液 （属专用阀门）","台","1.00","","","","","","推荐品牌：中国上正阀门/精工阀门/五洲阀门/良工阀门/立信阀门/无锡美瑞克；直发长青能化，报价包含运费，卸货费"]
["13","8225344204","截止阀","J41F-25P FM DN20 适用温度≤150℃","介质 :氨水","台","1.00","","","","","","直发长青能化，报价包含运费，卸货费"]
["14","8226358006","法兰旋启式止回阀","H44W-150LB DN50 RF    CF8/304","","台","2.00","","","","","","直发长青能化，报价包含运费，卸货费"]
["","合计","","","","","","","","","","",""]
["注：A、报价：无税单价（运费、装卸费出卖人承担）。"]
[" B、质量标准：国标、行业标准、企标，并注明标准号。非标产品以双方认可的图纸、协议等为准。"]
[" C、请务必填写完整、清晰，否则报价无效，修改处签章。"]
[" D、 “报价单”视为合同附件，具有法律效应。"]
[" E、付款方式：电子承兑。"]