{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["询价单"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"询价单","index":0,"n_rows":15,"n_cols":13,"rows_kept":15,"cut":false,"hidden":false,"merged":[[1,0,1,3],[1,6,1,11],[2,0,2,3],[2,6,2,11],[3,0,3,3],[3,6,3,11],[4,0,4,3],[4,6,4,11],[0,0,0,11]],"flags":["formulas_cached_only"]}
["徐州长城基础工程有限公司物资采购询（报）价单"]
["报价单位（公章或合同章）:",{"$nulls":5},"询价部门："]
["联系人:",{"$nulls":5},"联系方式："]
["传真:",{"$nulls":5},"报价截止日期："]
["供应商编码:"]
["序号","物资编码","物资名称","规格","型号","计量单位","数量","交货期","主机","无税单价（元）","总价（元）","品牌","备注"]
["1","TM20250606171938560d80e","屋面更换","屋面板更换预计2000m2（屋面板甲供）内容包括原屋面如需拆除自行考虑，拆除材料堆放指定地点；因场地狭小，上下料、人工二次倒运、脚手架、高空作业安全措施费等自行考虑；厂房内地面、墙面满铺防尘网自行考虑。","技术要求：符合国家及行业有关规范、标准，铁皮包边和型钢乙方自行考虑。","㎡","2000.00","","","","","","工期要求：15天"]
["2","TM20250606171938561d457","窗户更换","2、窗户更换预计200m2（窗户甲供）内容包括；拆除原有窗户；原墙面、墙体不得破坏且满足安装新窗户要求；厂房地板需满铺厚粘毯保护；墙板铁皮包边、C型钢、脚手架、防尘网等其他安全文明措施费自行考虑。","技术要求：符合国家及行业有关规范、标准，铁皮包边和型钢乙方自行考虑。","㎡","200.00","","","","","","工期要求：15天"]
["3","TM20250606171938562b8ad","窗户维修","窗户维修预计400m2内容包括：包含加固、打磨、清理、防腐、补胶、更换五金件、密封条等；厂房地板需满铺厚粘毯保护；墙板铁皮包边、C型钢、脚手架、防尘网等其他安全文明措施费自行考虑。","技术要求：符合国家及行业有关规范、标准，铁皮包边和型钢乙方自行考虑。","㎡","400.00","","","","","","工期要求：15天"]
["","合计","","","","","","","","","","",""]
["注：A、报价：无税单价（运费、装卸费出卖人承担）。"]
[" B、质量标准：国标、行业标准、企标，并注明标准号。非标产品以双方认可的图纸、协议等为准。"]
[" C、请务必填写完整、清晰，否则报价无效，修改处签章。"]
[" D、 “报价单”视为合同附件，具有法律效应。"]
[" E、付款方式：电子承兑。"]